# HRD Change Log

Created 25/05/2007 08:46:21.

| Version | Date | Component | Title | Status | Description
û | 3.5 b1489 | 25/05/2007 | HRD | DDE | Split Mode | Add Split Mode support via DDE, required when integrated via the DDE bridge. "The root cause here is that HRD's DDE interfaces do not include the ability to set or clear Split, or to set VFO B's frequency and mode; see http://hrd.ham-radio.ch/ddeinterfaces.html . As a result, the DXLab-HRD Bridge cannot command HRD to set or clear Split, or set VFO B's frequency and mode. As a result, when the user double-clicks on a DX Spot whose notes include a QSX frequency, SpotCollector cannot direct HRD to properly configure the transceiver to work the spotted station. Dave, AA6YQ
û | 3.5 b1463 | 29/04/2007 | CAT Commands | TX | Add | Is there a way to make the COM Port TX function in HRD / F8 / COM Port TX work for radios not in the list? Or a way to add radios to the list?
û | 3.5 b1448 | 14/04/2007 | HRD | TS-2000 MBC |  | Check manual beat canceller working.
û | 3.5 b1441 | 07/04/2007 | HRD | OMNI-VII | Add | Add OMNI-VII support.
û | 3.5 b1426 | 23/03/2007 | HRD | TS-2000 | To-Do | Simon, Thanks for the work on the TS-2000; it's good to be able to get at the memories and sub receiver now. I have, however, noticed some strange behaviour when switching between VFO's A & B while using 3.5 Beta: ## VFO A When the 'VFO A' button is pressed all is OK; the 'A' frequency appears on the main readout and the 'B' on the secondary readout. At this point, if the 'A/B' button is pressed the rig changes frequency and the main and secondary readouts are transposed as you would expect. Strangely, though, the 'VFO A' button remains illuminated and the 'VFO B' dark. ## VFO B When the 'VFO B' button is pressed, however, the secondary readout sticks on the 'B' frequency. Rig frequency and main readout change as expected. Thus the rig is left with VFO B displayed twice. The 'A/B' button does nothing! ## This behaviour happens on all clients and also when the server PC is used to control the rig directly. I've always been unable to use HRD's direct frequency entry mode for VFO B; that erratic behaviour seems to have spread to the buttons. Re-loading 3.4 returns the button behaviour to normal (direct entry still strange). ## G3YXM and G4FPH have noticed this as well, so it's not just down to my system! Another 'funny' carried over from 3.4 is that when the 'MBC' button is pressed it doesn't 'light up' but the Manual Beat Cancel IS activated. The only way to switch off 'MBC' is to press 'BC' twice (on then off again). Thanks again for the smashing software. I hope this helps. 73, de Phil, GJ4CBQ.
û | 3.5 b1426 | 23/03/2007 | HRD | VISTA | Bug | Simon: I was playing around with Windows Vista Enterprise recently. I installed it using a spare hard drive that I had. So basically, the computer hardware configuration that I was using was the same as used by my Windows XP installation. I installed HRD (latest from DM780 area). Installation ran fine. HRD starts up OK. But when trying to connect to the radio, HRD no longer would enumerate all of my "virtual" serial ports. Running under XP all 8 virtual ports are listed, but running under Vista, HRD doesn't show them. Just something to keep in mind when/if you ever officially support Vista. No hurry on that, since I didn't really see anything about Windows Vista that I liked!! __________________ 73, Michael Roland N9XY
û | 3.5 b1424 | 21/03/2007 | HRD | SDR-1000 | To-Do | January 3, 2006 Revisions: Corrected typo in MD. Changed ZZMD to reflect DIGU and DIGL. Added ZZTH and ZZTL commands. February 25, 2007 Revisions Added DN and UP commands. Added special codes in ZZST for new console step size frequencies. Corrected various typos. March 20, 2007 Revisions: Added: ZZAR AGC RF GAIN ZZBR BCI REJECTION ZZCB BREAK IN ENABLE ZZCD BREAK IN DELAY ZZCF SHOW CW TX FREQ ZZCI IAMBIC ON/OFF ZZCM CW MONITOR ON/OFF ZZCT COMPANDER THRESHOLD VALUE ZZGE NOISE GATE ENABLE BUTTON ZZGL NOISE GATE LEVEL VALUE ZZSR SPUR REDUCTION ON/OFF ZZTF SHOW TX FILTER ZZVA VAC ON/OFF ZZVE VOX ENABLE ZZVG VOX GAIN VALUE ZZXT X2TR ON/OFF Updated: ZZFI (DSP Rx Filters) to reflect current console values. (Dictionary update only, no change to CAT code).
û | 3.5 b1424 | 21/03/2007 | HRD | TS-2000 Support | Bug ? | Hi Simon; Thanks for the upgrades to the TS-2000 program. We have a local net every Tuesday for the TS-2000 and HRD--we can't get the SUB button to activate the sub transceiver. What are we missing? Randy W9RTB
û | 3.5 b1423 | 20/03/2007 | HRD | Modes | Bug | Simon, not really a 3.5 bug (been around a while), but: Some modes get passed thru the Virtual Serial Ports incorrectly. For example, K2 RTTY (mode value 6) and RTTY-R (mode value 9) get passed thru as USB (mode value 2). (K2 RTTY is really a data mode, not "true" RTTY). In the IC-746 Pro, RTTY gets passed thru as LSB (see http://forums.ham-radio.ch/showthread.php?t=6366). I don't know if this is an HRD issue or an N8VB issue (if N8VB, probably not much could be done about it), but as long as you're twidling with HRD's innards, maybe you could take a quick look at this? More of an annoyance really, but appears to affect multiple rigs (I had thought it was only an issue w/Elecraft K2s). TNX. BTW, K2 RTTY is LSB, while RTTY-R is USB.
û | 3.5 b1423 | 20/03/2007 | HRD | TS-480SAT | To-Do | Can't select or see Memory Channels 0-99 nor freq(s), nor Alpha Tags. Special Memory Range Channels 90-99 inop. No Entry means for Memory Channel Alpha Tags. Rig switching from VFO to Mem mode only changes button in HRD from VFO to Mem -- freq does not update in HRD. HRD needs Direct Access Buttons for: 1) TS-480SAT Extended Menus; Access and Configuration 2) Memory Channel Management 3) DSP Defeat Monitor toggle 4) Squelch Defeat Monitor toggle 5) Up and Down for stepping through Memory Channels (also works on rig to step through Bands) 6) Mem=>VFO HRD needs direct Direct Entry Field for: 1) Memory Channel Number 2) Alpha Tag Meter should display S-Unit/PWR plus ALC, SWR and Comp. Mode (USB, CW, etc) should be displayed near freq. -- not only on mode set button. Use 4 buttong instead of 5 and Save one button by changing: VFO A, VFO B, TX-A, TX-B, A=B dedicated buttons to VFO A/B toggle, Split On/Off toggle, A=B, Mem=>VFO
ü | 3.5 b1400 | 25/02/2007 | HRD | TS-2000 ATT | Done | Fixed TS-2000 ATT button logic.
ü | 3.5 b1396 | 21/02/2007 | HRD | Elecraft A/B, A>B, B<A | Done | Added A/B, A>B, B<A for the mighty Elecraft K2.
û | 3.5 b1396 | 21/02/2007 | HRD | Kenwood A/B, A>B, B<A | Done | Added A/B, A>B, B<A for all Kenwood radios.
ü | 3.5 b1394 | 19/02/2007 | HRD | CAT Command Manager | Done | Reworked to make less noisy.
ü | 3.5 b1394 | 19/02/2007 | HRD | Macros Manager | Done | Reworked to make less noisy.
û | 3.4 b1379 | 04/02/2007 | HRD | Satellites | In Progress | Repairing the Satellite Tracking interface.
ü | 3.4 b1378 | 03/02/2007 | HRD | Skinning | Done | Added skinning to HRD, selected in the F8 Program Options.
ü | 3.4 b1372 | 28/01/2007 | HRD | TS-2000 | Done | Added Main and Sub buttons.
ü | 3.4 b1372 | 28/01/2007 | HRD | TS-2000 | Done | Made the extended menu dialog modal instead of modeless.
ü | 3.4 b1372 | 28/01/2007 | HRD | Appearance (Themes) | Done | Modified the themes programming and default appearance to use common code; this is shared with Digital Master 780. Provices product uniformity and less confusion for the poor old progammer. The users will appreciate this as well!
ü | 3.4 b1371 | 27/01/2007 | HRD | CPU Reduction | Done | Reduced CPU usage by simply overriding CWinApp::IsIdleMessage.
ü | 3.4 b1370 | 26/01/2007 | Scanning | Resume Times | Done | Added many more resume times for scanning.
ü | 3.4 b1370 | 26/01/2007 | HRD | Kenwood Memories | Done | Reworked the Memory Edit window
ü | 3.4 b1370 | 26/01/2007 | HRD | TS-2000 | Done | Added standard Scan button (SC0, SC1) ehich is easier to use than selecting Scan from the Various menu.
ü | 3.4 b1369 | 25/01/2007 | HRD | TS-2000 | Done | Removed RX Pri and TX Pri, replaced with Pri (FR3)
ü | 3.4 b1369 | 25/01/2007 | HRD | TS-2000 | Done | Added a Mem button (FR2).
ü | 3.4 b1369 | 25/01/2007 | HRD | TS-2000 | Done | Prompt user to power-off the TS-2000.
ü | 3.4 b1346 | 02/01/2007 | HRD | WinKeyer USB | To-Do | Make sure all values are within range when updating.
û | 3.4 b1346 | 02/01/2007 | HRD | WinKeyer USB | To-Do | The Standalone editor is bad when used with the numeric fields.
ü | 3.4 b1325 | 12/12/2006 | HRD | Advanced Menu | Done | Fixed problem with Advanced entries being in wrong dropdown bar.
û | 3.4 b1279 | 27/10/2006 | Logbook | Review | To-Do | Look at LogbookAnalysisView line 554 astrTmp.AddStg(_T("%s %s"), rcd.DateStart(), + rcd.TimeStart());
û | 3.4 b1274 | 22/10/2006 | CGetWebPage | Bug in Biog | Bug | Very probably a fatal bug parsing QRZ.com data via CGetWebPage, error is when getting biography info. int nMyLine = nLine; nMyLine++; if ((astrLines.GetSize() > nMyLine) && (astrLines[nMyLine].Find(_T("<p>")) == 0)) { ... AND // // Now hunt for > without a < following. // int nStart = 0; int nLength = 0; // // SJB 23-10-2006. // for (int nChar = nPosn + strToken.GetLength(); nChar < (strLine.GetLength() - 1); nChar++) { ...
û | 3.4 b1274 | 22/10/2006 | Logbook | ADIF Import | To-Do | Check for duplicates
û | 3.4 b1255 | 03/10/2006 | Shortwave Database | New Format | To-Do | Switch away from ILG. DeluxeSimon - have you heard that the ILG database may no longer be available. According to another group I belong to the web site has been under various pressures that have resulted in its closure - at least in the short time and maybe permanently.
û | 3.4 b1255 | 03/10/2006 | DX Cluster | New Bands | To-Do | Add 5MHz and 505kHz - 510kHz.
û | 3.4 b1251 | 29/09/2006 | PSK31 Deluxe | Cursor Problem | To-Do | I was able to confirm the symptom on my other computer. Here is the sequence of events that cause and correct this in my environment. I am running XP PRO, 2000+ AMD with 1 GB memory of bothe mactines with a FIC M/B SIS IO set. 1. start with a fresh install of HRD and PSK31, in this case Build 1241. 2. Start HRD and just do whatever. 3. Start PSK31 from HRD.. 4. In PSK use a macro to reply to QSO (XMT Immediately) CALL CALL de MY CALL MYCALL ( at this point the cursor is not in the text box and must be moused and dropped there. 5.. to fix the problem start over with PSK31 running first and call HRD from the PSK31 program. Everything will behave normally now. I don't know if this helps or confuses the issue Simon, hopefully it helps. It is really strange and I wonder if it is something I am doing (or perhaps not doing in setup)
û | 3.4 b1251 | 29/09/2006 | HRD | Crash Dumps | To-Do | Advice users about FTP
û | 3.4 b1251 | 29/09/2006 | HRD | Remote Server | To-Do | Don't power-down when using remote server.
û | 3.4 b1250 | 28/09/2006 | HRD | DX Cluster Submit | To-Do | When submitting a DX spot tell user that spots submitted to OH2AQ are only displayed on the OH2AQ cluster.
û | 3.4 b1249 | 27/09/2006 | HRD | CAT Commands | To-Do | Help text should be 'Elecraft, Kenwood & FT02000 & FTDX-9000'.
û | 3.4 b1249 | 27/09/2006 | HRD | Schemes | To-Do | Make sure new K2 scheme is shipped
û | 3.4 b1249 | 27/09/2006 | HRD | Main Tabs | To-Do | If main tabs are not shown make sure MDIClientWnd is used.
û | 3.4 b1249 | 27/09/2006 | Remote Server | Config File | To-Do | Make sure latest HRDRemoteServer.cfg is shipped, file location is: D:\Ham Radio\Release
ü | 3.4 b1249 | 27/09/2006 | HRD | Codejock Library | Done | Upgraded the Codejock library to 10.3.1 which fixes a few minor drawing errors.
ü | 3.4 b1248 | 26/09/2006 | HRD | Logbook | Done | Crash in print preview if Main Tabs are not displayed. Fixed in void CMainFrame::OnSetPreviewMode().
û | 3.4 b1247 | 25/09/2006 | HRD | Google Earth | To-Do | On a whim, I thought I might open up the DX Cluster_main.kml file. I followed the link to the DX Cluster.kml file and opened it up just fine with Google Earth. All the DX Cluster stations were identified with numbers and their callsign. Looking at the error message, I think I found the problem: One of the subfolders that contain the file has the & character as part of the name, no underline of course. This is the point at which the error occurs. I'm guessing Google Earth does not know what to do with it?? I tried to change the name of the folder, but since it is a Windows system folder, I cannot change it easily. Simon, can you think of a workaround for this? I guess I could just create a shortcut that points to the specific kml file. C:\Documents and Settings\Mom & Dad\Application Data\Simon Brown, HB9DRV\Ham Radio Deluxe
û | 3.4 b1242 | 20/09/2006 | HRD | Cluster Problem | Bug | I have some problems with cluster and the logbook. When i have added a new station in the logbook i can't make the scroll function to work in the cluster. I have to use the arrows in the left side. The only way to get it work again is to restart the software.
û | 3.3 b1236 | 14/09/2006 | HRD | Build 1235 Crash | Bug | Startup crash reported with 1235.
ü | 3.3 b1236 | 14/09/2006 | HRD | Change Log | Done | Double-click disabled unless HB9DRV.
û | 3.3 b1236 | 14/09/2006 | HRD | BugTrap | To-Do | Explain how to send report using FTP.
û | 3.3 b1235 | 13/09/2006 | HRD | IC-703 | To-Do | I am having problems with hrd displaying alc / swr / pwr it will work ok when in memory mod on my radio my radio is a icom ic-703 and the interface I am using is from zlp electronics is this a bug in hrd our am I doing something wrong?
û | 3.3 b1235 | 13/09/2006 | Logbook | Double Lines | Bug | Build 1227 still generates dbl horizontal grid lines in the Large Logbook display. See fullsize image via thumbnail below. The dbl lines occurred by clicking the downpointing scroll button to the lower right of the large logbook window. With each successive click of the buttons more records scrolled upward (the table scrolled downward) and the newly appearing records at the bottom of the logbook window showed the dbl horizontal lines.
ü | 3.3 b1235 | 13/09/2006 | Logbook | Autofill from QRZ | Done | Broken when adding code to close down background threads! Fixed!
ü | 3.3 b1235 | 13/09/2006 | Logbook | Cabrillo Help | Done | Added Cabrillo help to the Cabrillo Export window.
ü | 3.3 b1234 | 12/09/2006 | Logbook | eQSL.cc | Done | Bug - uploads times using local (if selected) and not GMT/UTC, now fixed.
ü | 3.3 b1234 | 12/09/2006 | Logbook | Cabrillo | Done | Added support for 'ARRL VHF contests and CQ VHF Contest' see http://www.kkn.net/~trey/cabrillo/qso-template.html . Note - all fields in a Cabrillo record are taken from the correspodning logbook record, so this record must contain My Station's Locator and My Station's Callsign. If missing these fields can be edited via the bulk editor.
ü | 3.3 b1233 | 11/09/2006 | Logbook | ARRL Sections | Done | Added Illinois
ü | 3.3 b1230 | 08/09/2006 | HRD | TS-480 baud Rate | Done | Added 4,800 for WB5OMP.
ü | 3.3 b1227 | 05/09/2006 | HRD | Closedown | Done | Resolve hang closing the 3rd-party serial ports if the driver in use does not honour timeouts. See void CEmulComPortThread::CloseDown() . The solution applied here should also resolve hangs with the DX Cluster when closing.
û | 3.3 b1227 | 05/09/2006 | HRD | WinKey | To-Do | Add macros features: [*] Enabled [*] Save to / Load from file.
ü | 3.3 b1224 | 02/09/2006 | HRD | Startup Diagnostics | Done | When starting a new connection (where you fill in the fields: Company, radio, Port etc.) I now display a log as the startup sequence is initiated.
ü | 3.3 b1224 | 02/09/2006 | HRD | Restart Radio Crash | Done | Found and resolved long-standing problem restarting with same radio - errors in the selection window advanced area.
ü | 3.3 b1221 | 30/08/2006 | HRD | IC-7000 | Done | I have found the following commands wrong in the 1C-7000 manual and as such are wrong in HRD resulting in some strange results. The correct commands are as follows: TX SSB bandwidth cmd=1a-06 not cmd=06 DSP filter shape cmd=1a-07 not cmd=07 Manual notch filter 1 cmd=1a-08 not cmd=08 Manual notch filter 2 cmd=1a-09 not cmd=09 Could we please include the following missing buttons: On/off button Attenuate Att-off cmd=11-00, Att-on cmd=11-12 The Mch pull down box to access the memory channels is also unavailable for the ic-7000 but is available for the 756proIII. Thanks for such a great product.
û | 3.3 b1220 | 29/08/2006 | HRD | Orion II | To-Do | Check the ORION II firmware for changed S-Meter and other new / ehanced commands.
ü | 3.3 b1220 | 29/08/2006 | Logbook | Future Dates | Done | Fixed problem where the message "The start and/or end date is in the future" is displayed, however the neither the start or end date is. Due to a bug when the user is displaying date/time using Local rather than UTC/GMT.
ü | 3.3 b1220 | 29/08/2006 | HRD | Closedown | Done | Close the serial port thread (used for 3rd party serial port support) when closing HRD - if not closed can cause a crash of HRD.
ü | 3.3 b1220 | 29/08/2006 | HRD | Donations | Done | Add 'Donations' button to the About window and the DX Cluster.
ü | 3.3 b1220 | 29/08/2006 | HRD | Change Log | Done | When creating the smaller kit make sure the Change Log HTML is shipped.
ü | 3.3 b1219 | 28/08/2006 | HRD | IC-746Pro | Done | Added: 1A-07 SSB transmit bandwidth (Wide, Medium, Narrow) 1A-08 DSP filter shape The buttons are: TX-Wide, TX-Mid, TX-Nar and Sharp.
ü | 3.3 b1217 | 26/08/2006 | HRD | Bands Popup | Done | Replace bands popup with a menu - less clicks & more consistent. Shown when clicking on the Bands Title in the tuning area.
û | 3.3 b1217 | 26/08/2006 | HRD | Bands Crash | Bug | Bands-related crash reported by OZ1TMK, Torben Mellerup <oz1tmk@oz1tmk.dk>
ü | 3.3 b1215 | 24/08/2006 | HRD | Selection Window | Done | Fixed bug reported by G6CNQ with IC-756 ProII.
ü | 3.3 b1214 | 23/08/2006 | HRD | Main Tabs | Done | Added a context menu.
ü | 3.3 b1213 | 22/08/2006 | HRD | Display Crash | Done | Fixed fatal error drawing tuning bands as reported by OZ1TMK.
ü | 3.3 b1213 | 22/08/2006 | HRD | Selection Window | Done | Changed underlying code used to display the Selection window.
û | 3.3 b1213 | 22/08/2006 | HRD | Advanced Sliders | To-Do | Optimise refresh of sliders in an Advanced list by sending all requests in one packet, especially for remote operation.
û | 3.3 b1209 | 18/08/2006 | Logbook | ALE Reset | To-Do | When Autofill is enabled pressing Reset does not cancel the autofill.
ü | 3.3 b1208 | 17/08/2006 | Serial Port Server | Timeouts | Done | Increased timeouts to 2 seconds to avoid hideous latency problems encountered by some users.
ü | 3.3 b1208 | 17/08/2006 | HRD | DX Cluster | Done | Changed default Distance from miles to kilometers.
ü | 3.3 b1208 | 17/08/2006 | HRD | Toolbar Text | Done | Toolbar text can be shown / hidden via the 'Toolbar Text' option in the View menu. Update: sticky everywhere now, including Logbook.
ü | 3.3 b1208 | 17/08/2006 | HRD | Startup | Done | Optionally start logbook when connecting to radio.
ü | 3.3 b1208 | 17/08/2006 | HRD | Main Tabs | Done | Using the Logbook's Print-Preview causes docking panes to lose their contents. Fixed - just ignore special print-preview processing for now.
ü | 3.3 b1208 | 17/08/2006 | HRD | Docking Panes | Done | Docking panes are now sticky - an affinity with monitor an application edges.
ü | 3.3 b1208 | 17/08/2006 | HRD | Docking | Done | Making docking windows sticky (Codejock 10.3).
ü | 3.3 b1208 | 17/08/2006 | HRD | Change Log | Done | Non-HB9DRV users only see HTML.
ü | 3.3 b1208 | 17/08/2006 | Logbook | Toolbar | Done | Only show one Add entry in the Logbook Toolbar, the other two should be hidden.
ü | 3.3 b1208 | 17/08/2006 | HRD | Sliders | Done | By default the sliders in the Selection/Advanced window now use the custom design.
ü | 3.3 b1208 | 17/08/2006 | Logbook | Modes | Done | Fixed Modes problem introduced in build 1207.
û | 3.3 b1208 | 17/08/2006 | HRD | Main Tabs | To-Do | [1] Add popup context menu for Main Tabs. [2] Optionally display Main Tabs in Full Screen mode.
ü | 3.3 b1208 | 17/08/2006 | HRD | View Menu | Done | Redesigned the View menu.
ü | 3.3 b1208 | 17/08/2006 | HRD | Main Tabs | Done | Updated Main Tabs logic, see F8 Settings / Theme.
û | 3.3 b1208 | 17/08/2006 | Logbook | Daily Counter | To-Do | Add daily QSO counter
ü | 3.3 b1207 | 16/08/2006 | HRD | Change Log | Done | Changed HTML title to 'HRD Change Log'.
ü | 3.3 b1207 | 16/08/2006 | HRD | Toolbars | Done | Toggle the display of toolbar text with the new 'Toolbar Text' option in the View menu. Added 'Customise Toolbars' to the View menu.
ü | 3.3 b1207 | 16/08/2006 | HRD | Main Tabs | Done | Redesigned the Main Tabs implementation.
ü | 3.3 b1207 | 16/08/2006 | HRD | Themes | Done | Reworked the F8 Sttings Themes options.
û | 3.3 b1205 | 14/08/2006 | HRD | Winkeyer | To-Do | When defining a memory replace / with // or at least warn user that it's a special case character.
û | 3.3 b1205 | 14/08/2006 | HRD | Startup | To-Do | Optionally start Analysis when connecting for first time.
û | 3.3 b1205 | 14/08/2006 | HRD | Pane Manager | To-Do | Change layout from xtpTabLayoutSizeToFit to xtpTabLayoutAutoSize, this will add scroll buttons (requested by Terry).
ü | 3.3 b1205 | 14/08/2006 | HRD | Toolbar Text | Done | Make toolbar text optional
ü | 3.3 b1205 | 14/08/2006 | HRD | Main Tabs | Done | Added main tabs (See View menu) - this is experimental.
û | 3.3 b1203 | 12/08/2006 | HRD | Steps Sizes | To-Do | Add 125 kHz.
û | 3.3 b1203 | 12/08/2006 | Logbook | Add / Maximise | To-Do | If attempting to maximise the Add / Edit window with Advanced controls switched off give audible error indication or (better) disable Maximise window. At least don't confuse the users.
ü | 3.3 b1202 | 11/08/2006 | HRD | Change Log | Done | Check HTML created in correct folder.
ü | 3.3 b1201 | 10/08/2006 | Logbook | Location Distance | Done | Support kilometers and miles (metric and imperial) in the Location tab of the Add / Modify logbook entry. The values stored in the database is always kilometers.
ü | 3.3 b1201 | 10/08/2006 | Logbook | Totals | Done | Show x / y where y is the total in the database, not the maximum selected for display.
ü | 3.3 b1200 | 09/08/2006 | HRD | Change Log | Done | Added current filename to the Change Log display.
ü | 3.3 b1200 | 09/08/2006 | HRD | Quick Save Crash | Done | Selecting Erase All from the Quick Save menu would cause a crash as the markers were not erased correctly. Changes made to CMainFrame::OnQuickEraseAll() and CRadioView::OnRefreshDial().
ü | 3.3 b1199 | 08/08/2006 | Logbook | Bug fixes | Done | Fixed minor bugs resulting from yesterday's work.
ü | 3.3 b1198 | 07/08/2006 | Logbook | Add - Icons | Done | Added icons to the Logbook pane, clicking on the icon changes the icon. Designed for use with nets, the icon is volatile (not saved in the database). Added at the request of a keen logger of nets.
û | 3.3 b1198 | 07/08/2006 | HRD | BugTrap | To-Do | Call BT_SetTerminate() in every thread (see page 24 of the doc).
ü | 3.3 b1197 | 06/08/2006 | Logbook | Modes | Done | Added more modes, the list of modes confirms to ADIF spec 2.1.17 . to load the latest list: start the Logbook, select Configure, select List - Modes and press Reset.
ü | 3.3 b1197 | 06/08/2006 | HRD | AOR | Done | Added AOR support to the Command Tester, specifically tailored for the AOR-500. This is a test - this is not a promise that I will support AOR-5000 this millenium.
ü | 3.3 b1197 | 06/08/2006 | Logbook | Add | Done | The Add Logbook Entry window has been extended: * It is resizable, can be maximised. * The logbook pane supports Copy / Modify / Delete / End=Now (set end time to current time). So if you are running a net it's now much easier to keep track of the participants using just this window.
û | 3.3 b1197 | 06/08/2006 | HRD | Browser Pane Titles | To-Do | Browser pane titles can be too long, look at abbreviating if insufficient room.
û | 3.3 b1194 | 03/08/2006 | Logbook | QSL End Time | Bug | If the end time is set automatically and the user is displaying local time then the end time is local, not GMT. Look at OnEndTime() called from Add().
ü | 3.3 b1193 | 02/08/2006 | Logbook | eQSL.cc | Done | eQSL.cc now supports Satellite Mode and Propogation Mode if entered by the user. The real-time submit option in the Logbook menu now supports using the standard eQSl.cc test username and password (TEST-SWL / Testpswd).
ü | 3.3 b1193 | 02/08/2006 | HRD | Accelerators | Done | Menu accelerators lost.
ü | 3.3 b1193 | 02/08/2006 | Logbook | Reset | Done | If a callsign is entered and auto-QRZ is selected and the user presses Reset then the QRZ fields get loaded.
û | 3.3 b1193 | 02/08/2006 | Logbook | Autofill | To-Do | The Add and Edit logbook entry have a tab labeled Location. Now that we have a new cuntries list with CQ zone, ITU zone, etc., when using Configure/Update logbook, could you automatically fill/update the fields of this location tab? This location tab has a field (ARRL section) which is relevant only to US stations. Could it be changed to something else according to the country of the station contacted?
ü | 3.3 b1192 | 01/08/2006 | HRD | FT-2000 | Done | Added initial support for the new Yaesu FT-2000.
û | 3.3 b1192 | 01/08/2006 | Logbook | Modes | To-Do | Make Modes user-definable
û | 3.3 b1192 | 01/08/2006 | Logbook | Configure & Options | To-Do | Merge the Logbook Options into Logbook COnfigure sheet. Make it obvious where eQSL.cc info is held, add a eQSL.cc test option.
û | 3.3 b1192 | 01/08/2006 | Logbook | Navigation | To-Do | Make it easier to navigate between Analysis and Logbook
û | 3.3 b1192 | 01/08/2006 | Logbook | Worked | To-Do | Optionally display Worked even if worked on another band
ü | 3.3 b1192 | 01/08/2006 | Logbook | Transverters | Done | Load frequency from Transverter display if visible.
û | 3.3 b1192 | 01/08/2006 | Logbook | Reset on Close | To-Do | Optionally reset when closing [X]
ü | 3.3 b1192 | 01/08/2006 | Logbook | Archiving | Done | Logbook now supported by the Tools / Archive option even if it's not in the default HRD Settings Folder.
ü | 3.3 b1192 | 01/08/2006 | Logbook | Grid Lines | Done | Enabled grid lines option in the Logbook Configure window. By default grid lines are not shown. The grid lines are the defaults supported by the MFC CListCtrl control.
ü | 3.3 b1192 | 01/08/2006 | Logbook | My Station | Done | When the My Station data is updated with the Logbook Configure window then Add window is automatically updated.
û | 3.3 b1192 | 01/08/2006 | Logbook | Worked Status | To-Do | Always check the worked status, even if logbook tab not displayed.
ü | 3.3 b1192 | 01/08/2006 | Logbook | Audible Worked Status | Done | If a station has been worked then 'Station Worked' is spoken using text to speech.
ü | 3.3 b1192 | 01/08/2006 | Logbook | Defaults | Done | The frequency, band and mode are saved when an entry is added and used as the defaults when the window is opened. If a radio is connected when the Add window is open then the radio's values are used.
ü | 3.3 b1192 | 01/08/2006 | Logbook | ARRL Section | Done | ARRL Section is now cleared when the logbook window is reset.
ü | 3.3 b1192 | 01/08/2006 | Logbook | Add x 3 | Done | There are now 3 windows for adding logbook entries. The windows are selected from the Logbook menu and / or the Logbook toolbar. As a call is entered which adding an entry the callsign is also displayed in the window's frame.
û | 3.3 b1191 | 31/07/2006 | HRD | ICOM 751A | Bug | See http://forums.ham-radio.ch/viewtopic.php?p=24084&sid=59e0fe6e73a99210c8b11a969e8bde68#24084
ü | 3.3 b1191 | 31/07/2006 | Logbook | Country Data | Done | The country data is now held in table TBL_COUNTRIES_001, previously the table used was TBL_COUNTRIES. The data can now be edited by the user and saved to / loaded from XML files. There is also a Test option. To display the contents of the table select Configure from the Tools menu. The default data format is XML, prior to this build it was .txt .
ü | 3.3 b1188 | 28/07/2006 | HRD | User Guide | Done | Add User Guide and Change Log to Start menu
ü | 3.3 b1186 | 26/07/2006 | HRD | CGetWebPage::Get() | Done | Wrap all code in this member function inside a TRY and CATCH blocks to ensure all exceptions thrown by the internet functions are hopefully caught. Also the pointer returned from CInternetSession::OpenURL() is now deleted after being closed.
ü | 3.3 b1186 | 26/07/2006 | PSK31 Deluxe | CDisplyCanvas::Initialise() | Done | Changed size of variables m_anOffsetToPosVert and m_anOffsetToPosHorz to be actual window size, not internal area initially reserved for waterfall data. Crash caused by internal area growing when frequency changes and RF frequency is displayed rather than AF frequency. 27/07/2006 - confirmed as now fixed.
ü | 3.3 b1186 | 26/07/2006 | Logbook | Country File | Done | "Serbia and Montenegro" becomes simply "Serbia" and "Montenegro" is a new country since 28 jun 2006 ! The previously deleted "Swan Isl." with KS4, become a new country with KH4 ! Unfortunately some call that now belog to "Montenegro" like 403? or YU6?? remains as "Serbia and Montenegro" instead of "Montenegro" alone.
û | 3.3 b1186 | 26/07/2006 | HRD | FT-817 Codes | To-Do | Add buttons for turning break-in on and off (CW) as well as switching modes such as RTTY, USER-U and USER-L. Look at the FT-817 Commander windows DIG/PKT and CW.
û | 3.3 b1185 | 25/07/2006 | Logbook | eQSL.cc Download | To-Do | Add support for downloading from eQSL.cc
û | 3.3 b1185 | 25/07/2006 | Logbook | SWL Support | To-Do | Add expression in QSL Comment field of eQSL Upload. ex: For SWL use I have to manually edit the comment field for every QSO and add the correspondant Callsign. It would be nice to use expression: In QSO with + 'logbook_custom_field_1' to do all automatically!
ü | 3.3 b1185 | 25/07/2006 | HRD | eQSL.cc | Done | When uploading, at the end, eqsl.cc reports that HamRadioDeluxe is not being recognized. While asking eqsl.cc people, they told me that the program name in eqsl.cc's database supplied by Simon is "Ham Radio Deluxe" e.g. without spaces. Could this be changed (either way)? Note: seems to work OK.
û | 3.3 b1185 | 25/07/2006 | DX Cluster | Startup Scripts | To-Do | Startup scripts needed for the DX Cluster when connecting to a DX Spider.
ü | 3.3 b1185 | 25/07/2006 | HRD | Crash | Done | Added try catch exception handler in COXBitmapButton line 1464 to try stop some Windows 98 crashes.
ü | 3.3 b1184 | 24/07/2006 | PSK31 Deluxe | BugTrap | Done | Added bugtrap from http://www.intelle-soft.com/ into PSK31 Deluxe to produce meaningful crash support.
ü | 3.3 b1184 | 24/07/2006 | HRD | BugTrap | Done | Added bugtrap from http://www.intelle-soft.com/ into HRD to produce meaningful crash support.
ü | 3.3 b1183 | 23/07/2006 | HRD | Winkeyer | Done | Store macros in a XML file instead of Registry.
û | 3.3 b1183 | 23/07/2006 | HRD | Jupiter Tuner | To-Do | Add support for the Jupiter internal ATU if possible.
û | 3.3 b1183 | 23/07/2006 | HRD | TS-950 | To-Do | Add Filter, RIT/XIT.
û | 3.3 b1183 | 23/07/2006 | HRD | Save Tune Up Power Level | To-Do | Before the change: HRD Tune Up would change the mode (RTTY in my case) and reduce the power to a setting I choose. When clicking Stop and then Cancel, the power and mode would return to normal. The next time Tune Up is run, the lower power setting is still present. The power setting for regular operation is still at the normal level. After the change: Everything is the same as before the change, except that the lower power setting is not saved. I have to change it on the slider each time.
û | 3.3 b1183 | 23/07/2006 | HRD | Scanning | To-Do | Support squelch status for stopping scanning
û | 3.3 b1183 | 23/07/2006 | HRD | TS-940S | To-Do | Check the IF-10A / IF-10B manual for TS-940S support.
û | 3.3 b1183 | 23/07/2006 | DX Cluster | 5 MHz | To-Do | Add support for the 5 MHz band if possible.
ü | 3.3 b1183 | 23/07/2006 | HRD | Reset Options | Done | The Reset option in the File menu now supports moving all files from the application specific folder to a folder in the same tree with a timestamp, this clears all files from the folder but does not erase them. For example move all files from: C:\Documents and Settings\Simon\Application Data\Simon Brown, HB9DRV\Ham Radio Deluxe\ to: C:\Documents and Settings\Simon\Application Data\Simon Brown, HB9DRV\Ham Radio Deluxe 2006-Jul-23 101152\
û | 3.3 b1180 | 20/07/2006 | Winkeyer | USB Hang | To-Do | If the USB cable is unplugged and then plugged back in while a connection is open then closing the connection hangs.
ü | 3.3 b1180 | 20/07/2006 | PSK31 Deluxe | Crash | Done | Hello Simon, Right,this is how I had things setup: (a) Start HRD and connect to TS850. Everything works as it should - rig under HRD control etc. (b) Start PSK31 from the button on the HRD tool bar Now, before I go on I think I might have found some repeatability in the crashes. (c) PSK31 normally loads full screen and I resize it so I can see other software that I normally run - Wavenode Pwr/SWR meter for instance. Using the resized screen in classic channel 1, and clicking "Favourites down" (PSK31 top of screen << arrow) causes a crash and during tests this morning has been quite repeatable. However running PSK31 full screen, in classic channel 1, appears to have reduced the problem quite significantly - I have been moving up and down using the Favourites button << >> many times and only had one crash whereas with the resized screen it happens almost immediately. Does this shed any light on the problem area - can anyone else here confirm this behaviour? Trevor G0KTN
ü | 3.3 b1180 | 20/07/2006 | HRD | Change Log | Done | Changed logfile format from .txt to .xml .
ü | 3.3 b1179 | 19/07/2006 | HRD | Customise Layout | Done | Radio not part of default filename, when radio value is set the filename must be rebuilt. Remove code to put radio into page title.
û | 3.3 b1160 | 30/06/2006 | Logbook | XML | To-Do | Add XML support for loading tables
ü | 3.3 b1160 | 30/06/2006 | Logbook | New Country | Done | Add 514 Montenegro, change 296 Serbia
û | 3.3 b1159 | 29/06/2006 | CAT Commands | Fail To Load | To-Do | Mention that a HRD restart may be needed.
û | 3.3 b1159 | 29/06/2006 | CAT Commands | Fail To Load | To-Do | Fail to load CAT commands from a file.
û | 3.3 b1159 | 29/06/2006 | Help | Connect | To-Do | Improve the Connect Help text, include information about USB problems (lack of power, driver issues).
û | 3.3 b1159 | 29/06/2006 | Kenwood Support | More Support | To-Do | Add Memory Up/Down buttons.
û | 3.3 b1158 | 28/06/2006 | Closedown | DX Cluster Hangs | To-Do | Added a closedown watchdog thread to ensure that HRD closes even if the DX cluster or any other background thread is hanging.
ü | 3.3 b1157 | 27/06/2006 | Winkeyer | Winkeyer 2 | Done | Add support for Winkeyer 2 memories.
ü | 3.3 b1157 | 27/06/2006 | Winkeyer | Winkeyer 2 | Done | Added initial support for Winkeyer 2 (the new USB device).
ü | 3.3 b1157 | 27/06/2006 | HRD | Change Log | Done | *** Change log is overwritten when new kits are installed.
ü | 3.3 b1157 | 27/06/2006 | HRD | Change Log | Done | *** Change log added, only HB9DRV can update entries.